23/05/23

Nevus installation with Hydrological International

Lock at loggerbox 0023

Software PIN 2718

Order of things to do:

1. Download/save data
2. Clean reformat sd card
3. New setup – period internal (1 min sampling time)
4. Flow spot gauging, velocity index method
5. Download data
6. Clean reformat SD card
7. New setup – period internal (15 min sample time)

Rating curve point 23/05/23

0.17m, 0.020 m3s-1, no instream vegetation, only bankside veg.